

# Exercise 1 – Basic network stuff

Difficulty: **Easy**

**Task 1**: Use the arp command and paste the output from the arp table on your system:




**Task 2**: Use the route command and paste the output from the routing table on your system:



**Task 3**: Use the traceroute command on your system and observe the hops to Google’s DNS,

* + - 1. Paste the full output from the command bellow showing all the hops from your system to 8.8.8.8.



## Task 4: Why would you need to use the ping command?

Answer: To check if the connection is established successfully by sending a couple of packets and monitoring if they were received without any lost.

## Task 5: Write down the TCP/UDP ports of the most commonly used services bellow in the form of TCP[PORT] or UDP[PORT].

As an example, the first two answers have been filled in:

* + - * + HTTP - TCP80
        + SNMP - UDP 161
        + HTTPS - TCP 443
        + DNS - UDP 53 - Client
        + DNS - TCP 53 - Zone transfer
        + SMTP - TCP 25
        + SSH - TCP 22
        + FTP - TCP 21
        + Telnet - TCP 23
        + MSSQL - TCP 1433
        + MySQL - TCP 3306
        + PostgreSQL - TCP 5432
        + RDP - (Remote Desktop Protocol) TCP 3389
        + NTP - UDP 123
        + NFS - Uses port 2049 TCP or UDP port 111

# Exercise 2 – TCP/IP Basics

Difficulty: **Medium**

## Refer to the exhibit and answer the questions below.

## Task 1: For each of the packet locations shown, 1 to 4 write down the source and destination MAC addresses of the packet as it travels across the network interfaces.

1. **The laptop initiates communication with the web server and prepares a packet. What would the packet look like at this stage?**
   * **SRC IP 100.20.30.10**
   * **DST IP 80.70.60.100**
   * **SRC MAC AA:AA:AA:33:33:33**
   * **DST MAC BB:BB:BB:11:11:01**
2. **RTR1 receives the packet on its IF-LAN interface, prepares it accordingly and forwards it out its IF- WAN. What would the packet look like at this stage?**
   * **SRC IP 100.20.30.10**
   * **DST IP 80.70.60.100**
   * **SRC MAC BB:BB:BB:11:11:02**
   * **DST MAC CC:CC:CC:22:22:02**
3. **RTR2 receives the packet on its IF-WAN interface, prepares it accordingly and forwards it out via IF- LAN. What would the packet look like at this stage?**
   * **SRC IP 100.20.30.10**
   * **DST IP 80.70.60.100**
   * **SRC MAC CC:CC:CC:22:22:01**
   * **DST MAC DD:DD:DD:77:77:77**
4. **The web server receives the packet and prepares a response packet back. What would the packet look like at this stage?**
   * **SRC IP 80.70.60.100**
   * **DST IP 100.20.30.10**
   * **SRC MAC DD:DD:DD:77:77:77**
   * **DST MAC CC:CC:CC:22:22:01**

## Task 2: Since we are talking about web traffic (www) in the example, which transport layer protocol will most probably be used?

* TCP – Because is more reliable and ensures more positive results and most of the ports use it by default
* UDP

## If we do a traffic analysis with a network packet monitoring tool like WireShark, what can we expect to see for the source and destination ports when the laptop sends the packet?

* + - * + SRC PORT: temporary port
        + DST PORT: port 80

## Similarly, and vice versa, what can we expect to see as destination ports when the Web server sends a response packet back?

* + - * + SRC PORT: port 80
        + DST PORT: temporary port

**How many broadcast domains are there in the exhibit shown?**  4

There are two broadcast domains because the routers do not forward broadcasts from one of their interfaces to another so the bottom parts if the network inside the LAN are separate broadcast domains.

# Exercise 3 – Traffic analysis and identifying the OSI layers of the network packets


Difficulty: **Hard**

## Prerequisite:

Prerequisite: Search online and get familiar with the TCP’s three-way handshake. Learn how to capture the three way handshake using Wireshark. Install Wireshark on your computer and use it to capture traffic against a website or a server or your choice. It is recommended that you capture traffic against a simple website. Name and the IP address of the website you plan to capture traffic:

## Analyze the TCP’s three-way handshake and using screenshots from the Wireshark window answer the questions bellow:


1. What is the source IP (of the initiating host): The Source ip is my 192.168.0.102
2. What is the destination IP? (target website): 194.153.145.104 (abv.bg)




## Identify the Network Interface (Layer 1 & 2) section of the SYN packet and paste a screenshot from it:

## 

## Identify the Network Layer 3 section of the SYN/ACK packet and paste a screenshot from it:




## Identify the Transport Layer 4 section of the ACK packet and paste a screenshot from it bellow:



Look closely at the L2 section of the three-way handshake packet details. Each of them shows the source and destination MAC address of the packets.

**Who is the owner of the destination MAC address of the SYN packet?**

The owner is TendaTec\_bb:94:c8

****